|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Scouts_Australia-logo-E8934C8BDD-seeklogo | | SCOUT AUSTRALIA - SA BRANCH  INDIVIDUAL CANOE REGISTRATION FORM 2022  Note. All Canoes must be registered by the 1st September each year to be current.  Canoe is not registered until the decal is attached.  UNREGISTERED SCOUT SA OWNED CANOES ARE NOT INSURED OR COMPLY WITH THE NATIONAL MARITIME LAWS  Note – it is advantageous to permanently mark the Scout ID number on the Canoe in case the decal is detached. | | | | | | | | | Canoe  ID Number:  ScoutsSACanoe   |  | | --- | |  | |
| Date of inspection | | |  | | Group ID (if applicable) | |  | | Brand |  | |
| Surveyor’s Name | | |  | | Canoe/Kayak/Sit on | |  | | Seats |  | |  |
| District | | |  | | Length (M) | |  | | Serial Number |  | |
| Construction e.g plastic | | |  | | Colour Hull/Deck | |  | | Owner |  | |
| Inspected Item | Condition | | | | | | | Checklist | | | |
| Acceptable | | | Not Acceptable | | Not Applicable | |
| Hull/Deck |  | | |  | |  | | No Breaks, cracks or leaks | | | |
| Seams |  | | |  | |  | | Joints sound and smooth | | | |
| Patches |  | | |  | |  | | Secure, smooth and leak free | | | |
| Seats |  | | |  | |  | | Rigid, smooth, no splits & securely attached | | | |
| Coaming |  | | |  | |  | | Securely attached, smooth | | | |
| Footrest |  | | |  | |  | | If fitted secure, fail safe (Non trappable) | | | |
| Handgrips |  | | |  | |  | | Each end, 8 mm line minimum, toggles nominally 100mm x 25mm | | | |
| Buoyancy |  | | |  | |  | | Securely fixed, canoe floats flat when flooded | | | |
| Decklines |  | | |  | |  | | Securely attached, not slack | | | |
|  |  | | |  | |  | |  | | | |
| All items below that may be used with this craft have been checked: | | | | | | | | | | | |
| Inspected Item | Condition | | | | | | |  | | | |
| Acceptable | | | Not Acceptable | | Not Applicable | |  | | | |
| Paddle size/ type |  | | |  | |  | | Correct type and size for craft | | | |
| Paddle shaft |  | | |  | |  | | Smooth, no splits or corrosion, top hand grip secure. | | | |
| Paddle floatation |  | | |  | |  | | Must float level | | | |
| PFD |  | | |  | |  | | Appropriate for craft and must meet Australian Standard. | | | |
| Spraydecks |  | | |  | |  | | Release strap secure, no holes | | | |
| Bailer |  | | |  | |  | | Suitable bailer | | | |
| Comments: (If any Item is not acceptable – decal cannot be issued unless explanation is supplied). | | | | | | | | | | | |

Please return completed form to BC-Paddling via:

* Email – [paddlingsurveying@sa.scouts.com.au](mailto:paddlingsurveying@sa.scouts.com.au) OR
* Post to Scouts SA (please keep a copy & contact BC Paddling if no decal sticker is received within 28 days) Date Decal issued \_\_ /\_\_ /\_\_